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AI-generated content may be incorrect.]                                          Water Quality Report 2025: Drinking Water Analysis                
                                                                                     
 Harnett County Regional WTP (PWS ID# 03-43-045)
Harnett Regional Water is pleased to present the 2025 Annual Drinking Water Quality Report.  This report is a snapshot of last year's water quality and includes information regarding where your water is coming from, what it contains, and how it compares to standards set by regulatory agencies. Our constant goal is to provide you with a safe and dependable supply of drinking water.  We want you to understand the efforts we make to continually improve the water treatment process and protect our water resources.  We are committed to ensuring the quality of your water and providing you with this information, because informed customers are our best allies.  If you have any questions about this report or your water supply, please contact Tracy Tant at (910-893-7575 ext. 3245.)  We want our valued customers to be informed about their water utility.  If you want to learn more, please attend any of the regularly scheduled Harnett County Board of Commissioners meetings.  They are held on the first and third Monday of each month at the Harnett County Resource Center and Library at 455 McKinney Parkway in Lillington, NC.  The first meeting of the month is normally at 9:00 AM and the midmonth meeting normally begins at 6:00 PM. 
What EPA Wants You to Know
Drinking water, including bottled water, may be expected to contain at small amounts of some contaminants.  The presence of contaminants does not necessarily indicate that water poses a health risk.  More information about contaminants and potential health effects can be obtained by calling the Environmental Protection Agency’s (EPA) Safe Drinking Water Hotline (800-426-4791).
Some people may be more vulnerable to contaminants in drinking water than the general population.  Immunocompromised people such as people with cancer undergoing chemotherapy, people who have undergone organ transplants, people with HIV/AIDS or other immune system disorders, some elderly, and infants can be particularly at risk from infections.  These people should seek advice about drinking water from their healthcare providers.  EPA/CDC guidelines on appropriate means to lessen the risk of infection by Cryptosporidium and other microbiological contaminants are available from the Safe Drinking Water Hotline (800-426-4791).
If present, elevated levels of lead can cause serious health problems, especially for pregnant women and young children.  Lead in drinking water is primarily from materials and components associated with service lines and home plumbing.  Harnett County is responsible for providing high-quality drinking water but cannot control the variety of materials used in plumbing components.  When your water has been sitting for several hours, you can minimize the potential for lead exposure by flushing your tap for 30 seconds to 2 minutes before using water for drinking or cooking.  If you are concerned about lead in your water, you may wish to have your water tested.  Information on lead in drinking water, testing methods, and steps you can take to minimize exposure is available from the Safe Drinking Water Hotline or at http://www.epa.gov/safewater/lead.
The sources of drinking water (both tap and bottled water) include rivers, lakes, streams, ponds, reservoirs, springs, and wells.  As water travels over the surface of the land or through the ground, it dissolves naturally occurring minerals and, in some cases, radioactive material, and can pick up substances resulting from the presence of animals or human activity.
Contaminants that may be present in source water include microbial contaminants, such as viruses and bacteria, which may come from sewage treatment plants, septic systems, agricultural livestock operations, and wildlife; inorganic contaminants, such as salts and metals, which can be naturally-occurring or result from urban stormwater runoff, industrial or domestic wastewater discharges, oil and gas production, mining, or farming; pesticides and herbicides, which may come from a variety of sources such as agriculture, urban stormwater runoff, and residential uses; organic chemical contaminants, including synthetic and volatile organic chemicals, which are by-products of industrial processes and petroleum production, and can also come from gas stations, urban storm water runoff, and septic systems; and radioactive contaminants, which can be naturally-occurring or be the result of oil and gas production and mining activities.
To ensure that tap water is safe to drink, EPA prescribes regulations which limit the number of certain contaminants in water provided by public water systems. Food and Drug Administration (FDA) regulations establish limits for contaminants in bottled water, which must provide the same protection for public health.

Lead in Drinking Water
Lead can cause serious health problems, especially for pregnant women and young children. Lead in drinking water is primarily from materials and components associated with service lines and home plumbing. Harnett Regional Water  is responsible for providing high quality drinking water and removing lead pipes, but cannot control the variety of materials used in plumbing components in your home. You share the responsibility for protecting yourself and your family from the lead in your home plumbing. You can take responsibility by identifying and removing lead materials within your home plumbing and taking steps to reduce your family's risk. Before drinking tap water, flush your pipes for several minutes by running your tap, taking a shower, doing laundry or a load of dishes. You can also use a filter certified by an American National Standards Institute accredited certifier to reduce lead in drinking water. If you are concerned about lead in your water and wish to have your water tested, contact ttant@harnett.org (910-893-7575 ext. 3245). Information on lead in drinking water, testing methods, and steps you can take to minimize exposure is available at http://www.epa.gov/​safewater/​lead.

When You Turn on Your Tap, Consider the Source
The Water that is used by this system comes from the Cape Fear River, which is formed by the confluence of the Deep, and Haw River along the border between Chatham and Lee counties. We are a surface water treatment plant located at 310 West Duncan St. in Lillington NC.

This system purchases water from City of Dunn, (PWS# 03-43-010)  

Source Water Assessment Program (SWAP) Results
The North Carolina Department of Environment Quality (DEQ), Public Water Supply (PWSS) Section, Source Water Assessment Program (SWAP) conducted assessments for all drinking water sources across North Carolina. The purpose of the assessment was to determine the susceptibility of each drinking water source (well or surface water intake) to Potential Contaminant Sources (PCSs). 
The relative susceptibility rating for Harnett Regional Water (HRW) was determined by combining the contaminant rating (number and locations of PCSs within the assessment area) and the inherent vulnerability rating (i.e., characteristics or existing conditions of watershed and its delineated assessment area.) The assessment findings are summarized in the table below: 

Help Protect Your Source Water

Water systems are encouraged to use this report to inform consumers of source water protection actions that are in the planning stages or are already in place, to invite public participation in locally based source water protection efforts, and to provide tips on ways they can protect their source water. See below for suggested content and examples. 

· Protection of drinking water is everyone’s responsibility. You can help protect your community’s drinking water source(s) in several ways:
· Examples of Protection Actions 
1.Dispose of chemicals properly 
2.Take used motor oil to a recycling center 
3.Volunteer in your community to participate in group efforts to protect your source 
4.Etc. 



	SWAP Result Summary

	Source Name
	Susceptibility Rating
	
SWAP Report Date

	CAPE FEAR RIVER
	Moderate
	9/10/2020

	DUNN/CAPE FEAR RIVER
	Higher
	9/10/2020
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The Complete SWAP Assessment report for Harnett Regional Water may be viewed on the website:  https://www.ncwater.org/?page=600 Note that because SWAP results and reports are periodically updated by the PWS section, the results may differ from the results on the CCR. To obtain a printed copy of this report, please mail a written request to: Source Water Assessment Program - Report Request, 1634 Mail Service Center, Raleigh NC 27699-1634, or email request to swap@deq.nc.gov. Please indicate System Name (Harnett Regional Water) PWSID (03-43-045), and provide your name, mailing address and phone number. If you have any questions about the SWAP report, please contact the Source Water Assessment staff by phone at 919-707-9098.
It is important to understand that a susceptibility rating of “higher” does not imply poor water quality, only the systems’ potential to become contaminated by PCSs in the assessment area.

Tommy Burns (Director’s Corner)
  HRW experienced a very productive year in 2025. Harnett County continues to grow at an astounding pace with many new planned residential developments underway.   HRW is busy planning to accommodate this growth to ensure our ability to provide our customers with outstanding water and sewer service well into the future. In 2026, we will begin work on a new water treatment plant near Erwin that will supply Harnett County’s water needs well into the future. Additionally, all our existing residential and commercial water services now have new automated digital meters which do not require manual reading. All HRW customers could view and track water usage, receive notification of leaks, and learn tips to save money on their bills. This free service is part of our commitment to provide you with the best tools to manage your water use and bill. We encourage you to get started today by logging in to the WaterSmart portal with your mobile device or web browser. You can log on at https://hrwnc.watersmart.com.  There has been a lot of attention in the media lately concerning PFAS, which stands for per- and polyfluoroalkyl substances, which are a class of manmade chemicals present at low levels in most fresh water supplies, homes, offices, supermarkets- practically everywhere. These chemicals make consumer goods resistant to stains, grease, water, etc. and have been manufactured by companies for use in our consumer goods for years. problem lies in that they are impossible to avoid and are called 
 “Forever chemicals” because they are nearly indestructible. These chemicals have recently been found to pose risks to our health. The United States Environmental Protection Agency (EPA) in association with the North Carolina Department of Environmental Quality (NCDEQ) has tasked public water systems to develop ways to reduce these chemicals to a safe level. HRW has begun a pilot project to do just that and is working towards implementing additional methods to ensure that these chemicals will be safely removed from our water supply.

We are very proud of our record of environmental compliance as evidenced by this water quality report. We did not have any water quality violations and produced excellent water for our customers as always. Contact us by email or phone to get your water treatment questions answered. HRW is very fortunate to have such a fine group of water treatment professionals who strive daily to provide only the best drinking water to all our citizens. HRW will continue to serve the citizens of Harnett County and the surrounding region by supplying only the best of the most important commodities in the world, water.
Cryptosporidium

The Harnett County Regional Water Treatment Plant does voluntary quarterly monitoring of its source water for cryptosporidium. Cryptosporidium is a microbial parasite, which is found in surface water throughout the United States. Of the four quarterly test, we only had a detection in the second quarter with 0.09 total (Oo)cysts/liter) in the source water.
Cryptosporidium is a microbial pathogen found in surface water throughout the U.S. Although filtration removes Cryptosporidium, the most commonly-used filtration methods cannot guarantee 100 percent removal.  Current test methods do not allow us to determine if the organisms are dead or if they are capable of causing disease.  Ingestion of Cryptosporidium may cause cryptosporidiosis, an abdominal infection.  Symptoms of infection include nausea, diarrhea, and abdominal cramps. Most healthy individuals can overcome the disease within a few weeks. However, immuno-compromised people, infants and small children, and the elderly are at greater risk of developing life-threatening illness. We encourage immuno-compromised individuals to consult their doctor regarding appropriate precautions to take to avoid infection. Cryptosporidium must be ingested to cause disease, and it may be spread through means other than drinking water.

Additional Information
We routinely monitor for over 150 contaminants in your drinking water according to Federal and State laws. The following tables list the contaminants detected in the last round of sampling. The presence of contaminants does not necessarily indicate that water poses a health risk. Unless otherwise noted, the data presented in these tables are from testing done January 1 through December 31, 2025. The EPA and the State allow us to monitor for certain contaminants less than once per year because the concentrations of these contaminants are not expected to vary significantly from year to year.  Some of the data, though representative of the water quality, is more than one year old. In these tables you will find many terms and abbreviations you might not be familiar with.  To help you better understand these terms we’ve provided the following definitions: 

Action Level (AL) - The concentration of a contaminant which, if exceeded, triggers treatment or other requirements which a water system must follow.  
Herbicide – Any chemical(s) used to control undesirable vegetation.
Maximum Contaminant Level (MCL) - The highest level of a contaminant that is allowed in drinking water.  MCLs are set as close to the MCLGs as feasible using the best available treatment technology.
Maximum Contaminant Level Goal (MCLG) - The level of a contaminant in drinking water below which there is no known or expected risk to health.  MCLGs allow for a margin of safety.
Parts per million (ppm) or Milligrams per liter (mg/L) - One part per million corresponds to one minute in two years or a single penny in $10,000.
Parts per billion (ppb) or Micrograms per liter (ug/L) - One part per billion corresponds to one minute in 2,000 years, or a single penny in $10,000,000. 
Pesticide – Generally, any substance or mixture of substances intended for preventing, destroying, repelling, or mitigating any pest.
Level 1 Assessment - A Level 1 assessment is a study of the water system to identify potential problems and determine (if possible) why total coliform bacteria have been found in our water system.
Level 2 Assessment - A Level 2 assessment is a very detailed study of the water system to identify potential problems and determine (if possible) why an E. coli MCL violation has occurred and/or why total coliform bacteria have been found in our water system on multiple occasions.
Locational Running Annual Average (LRAA) – The average of sample analytical results for samples taken at a particular monitoring location during the previous four calendar quarters under the Stage 2 Disinfectants and Disinfection Byproducts Rule.
Maximum Residual Disinfection Level (MRDL) – The highest level of a disinfectant allowed in drinking water.  There is convincing evidence that addition of a disinfectant is necessary for control of microbial contaminants. 
Maximum Residual Disinfection Level Goal (MRDLG) – The level of a drinking water disinfectant below which there is no known or expected risk to health.  MRDLGs do not reflect the benefits of the use of disinfectants to control microbial contaminants.
Million Fibers per Liter (MFL) - Million fibers per liter is a measure of the presence of asbestos fibers that are longer than 10 micrometers. 
Nephelometric Turbidity Unit (NTU) - Nephelometric turbidity unit is a measure of the clarity of water.  Turbidity in excess of 5 NTU is just noticeable to the average person.
Not-Applicable (N/A) – Information not applicable/not required for that particular water system or for that particular rule.
Non-Detects (ND) - Laboratory analysis indicates that the contaminant is not present at the level of detection set for the particular methodology used.
Parts per trillion (ppt) or Nanograms per liter (nanograms/L) - One part per trillion corresponds to one minute in 2,000,000 years, or a single penny in $10,000,000,000.
Parts per quadrillion (ppq) or Picograms per liter (picograms/L) - One part per quadrillion corresponds to one minute in 2,000,000,000 years or one penny in $10,000,000,000,000.
Picocuries per liter (pCi/L) - Picocuries per liter is a measure of the radioactivity in water.
Running Annual Average (RAA) – The average of sample analytical results for samples taken during the previous four calendar quarters.
Treatment Technique (TT) - A required process intended to reduce the level of a contaminant in drinking water.
Variances and Exceptions – State or EPA permission not to meet an MCL or Treatment Technique under certain conditions




	Lead and Copper Contaminants

	
Contaminant (units)

	Sample Date
	Your Water
(90th Percentile)
	Number of sites found above the AL
	Range

Low    High
	MCLG
	AL
	Likely Source of Contamination

	Copper (ppm)
(90th percentile)
	August-September 2025
	0.111
	0
	0.0525 – 0.163
	1.3
	AL=1.3
	Corrosion of household plumbing systems; erosion of natural deposits

	Lead (ppb)
(90th percentile)
	August-September 2025
	
N/D
	0
	0 - 0
	0
	AL=15
	Corrosion of household plumbing systems; erosion of natural deposits

	The table above summarizes our most recent lead and copper tap sampling data.   If you would like to review the complete lead tap sampling data, please email us at TTant@harnett.org (910-893-7575 ext. 3245)


	Stage 2 Disinfection Byproducts (DBPs) Total Trihalomethanes (TTHM) and Haloacetic Acids (five) (HAA5)

	
Disinfection Byproduct
	Year Sampled
	
MCL Violation
Y/N
	Your Water
	Range

Low           High
	MCLG
	MCL
	Likely Source of Contamination

	TTHM (ppb)
	2025
	N
	40.0
	18.5 – 41.8
	N/A
	80
	Byproduct of drinking water disinfection

	HAA5 (ppb)
	2025
	N
	30.3
	14.3 – 29.8
	N/A
	60
	Byproduct of drinking water disinfection

	
Some people who drink water containing trihalomethanes in excess of the MCL over many years may experience problems with their liver, kidneys, or central nervous systems, and may have an increased risk of getting cancer Some people who drink water containing haloacetic acids in excess of the MCL over many years may have an increased risk of getting cancer.



	Other Disinfection Byproducts Contaminants

	
Contaminant (units)

	MCL
Violation
Y/N
	Your
Water
	Range
Low       High
	MCLG
	MCL
	Likely Source of Contamination

	Chlorite (ppm)
	N
	0.42
	0.06 – 0.64
	0.8
	1.0
	Byproduct of drinking water chlorination


	Disinfectant Residuals Summary

	Contaminant (units)

	MRDL Violation
Y/N
	Your Water
(RAA)
	Range
Low         High
	MRDLG
	MRDL
	Likely Source of Contamination

	Chlorine (ppm)
	N
	1.4
	0.3 – 3.7
	4
	4.0
	Water additive used to control microbes

	Chloramines (ppm)
	N
	2.57
	1.0 – 4.2
	4
	4.0
	Water additive used to control microbes

	Chlorine dioxide (ppb)
	N
	N/A
	0 - 398
	800
	800
	Water additive used to control microbes


	Radiological Contaminants

	
Contaminant (units)

	Sample Date
	MCL Violation
Y/N
	Your
Water (RAA)
	Range

Low    High
	MCLG
	MCL
	Likely Source of Contamination

	Radium 228 (pCi/L)
	10-12-21
	N
	1.1
	N/A
	0
	5
	Erosion of natural deposits


	Inorganic Contaminants

	
Contaminant (units)

	Sample Date
	MCL Violation
Y/N
	Your
Water (RAA)
	Range

Low    High
	MCLG
	MCL
	Likely Source of Contamination

	Fluoride (ppm)
	1-6-25
	N
	0.66
	N/A
	4
	4
	Erosion of natural deposits; water additive which promotes strong teeth; discharge from fertilizer and aluminum factories


	Turbidity

	
Contaminant (units)

	Treatment Technique (TT) Violation
Y/N
	Your Water
	MCLG
	

Treatment Technique (TT)
Violation if:

	Likely Source of Contamination

	Highest single turbidity measurement
	N
	.08
	N/A
	                            Turbidity  > 1  NTU
	Soil runoff

	Lowest monthly percentage of samples meeting turbidity limits
	
N
	100%
	N/A
	
Less than 95% of monthly turbidity measurements are <  0.3 NTU

	

	Turbidity is a measure of the cloudiness of the water. We monitor it because it is a good indicator of the effectiveness of our filtration system. The turbidity rule requires that 95% or more of the monthly samples must be less than or equal to 0.3 NTU.


	Total Organic Carbon (TOC)

	Contaminant (units)

	TT Violation Y/N
	Your Water
(lowest RAA)
	Range Monthly Removal Ratio
Low - High
	MCLG
	Treatment Technique (TT) violation if:
	Likely Source of Contamination

	Total Organic Carbon (TOC) Removal Ratio (no units)

	N
	1.18
	1.12 – 1.50
	N/A
	Removal Ratio   RAA <1.00 and alternative compliance criteria was not met
	Naturally present in the environment



	Other Miscellaneous Water Characteristics Contaminants

	
Contaminant (units)

	Sample Date
	Your
Water
	Range
Low                 High
	SMCL

	Sodium (ppm)
	1-6-25
	22.0
	N/A
	N/A

	Sulfate (ppm)
	1-6-25
	60.6
	N/A
	250

	pH
	1-6-25
	7.4
	N/A
	6.5 to 8.5

	The PWS Section requires monitoring for other misc. contaminants, some for which the EPA has set national secondary drinking water standards (SMCLs) because they may cause cosmetic effects or aesthetic effects (such as taste, odor, and/or color) in drinking water.  The contaminants with SMCLs normally do not have any health effects and normally do not affect the safety of your water.


	Unregulated Contaminants Monitoring Regulation (UCMR)

	
Contaminant (ppb)

	Sample Date
	Your Water
(average)
	Range

Low        High

	Perfluorobutanoic acid (PFBA)
	Jan – Sept 2025
	0.0048
	

	Perfluoropentanoic acid (PFPeA)
	Jan – Sept 2025
	0.0057
	0.0040 – 0.0069

	Perfluorohexanoic acid (PFHxA)
	Jan – Sept 2025
	0.0056
	0.0040 – 0.0071

	Perfluoroheptanoic acid (PFHpA)
	Jan – Sept 2025
	0.0035
	0.0033 – 0.0036

	Perfluorooctanoic acid (PFOA)
	Jan – Sept 2025
	0.0064
	0.0045 – 0.0077

	Perfluorobutanesulfonic acid (PFBS)
	Jan – Sept 2025
	0.0034
	

	Perfluorohexanesulfonic acid (PFHxS)
	Jan – Sept 2025
	0.0031
	0.0030 – 0.0031

	Perfluorooctanesulfonic acid (PFOS)
	Jan – Sept 2025
	0.0093
	0.0077 – 0.0123

	[bookmark: _Hlk215746565]Our water system has sampled for a series of unregulated contaminants. Unregulated contaminants are those for which EPA has not established drinking water standards. The purpose of unregulated contaminant monitoring is to assist EPA in determining the occurrence of unregulated contaminants in drinking water and whether future regulations are warranted. If you are interested in examining the results, please contact us at ttant@harnett.org.



	Water Quality Table(s) For City of Dunn PWS# 03-43-010  :2025
       (Purchased)



	
Contaminant (units)

	Sample Date
	Your Water 
(90th Percentile)
	Number of sites found above the AL
	Range

Low    High
	MCLG
	AL
	Likely Source of Contamination

	Copper (ppm)
(90th percentile)
	8/19-9/11/25
	0.09202 (ppm)
	0
	N/D-0.107 (ppm)
	1.3
	AL=1.3
	Corrosion of household plumbing systems; erosion of natural deposits 

	Lead (ppb)
(90th percentile)
	8/19-9/11/25
	N/D

	0
	N/D-3.8 (ppb)
	0
	AL=15
	Corrosion of household plumbing systems; erosion of natural deposits


Lead and Copper Contaminants

The table above summarizes our most recent lead and copper tap sampling data. If you would like to review the complete lead tap sampling data, please email us at Dunnwp@dunn-nc.org.
We have been working to identify service line materials throughout the water system and prepared an inventory of all service lines in our water system.To access this inventory, A hard copy will be made available for  review at City Hall. Lead can cause serious health problems, especially for pregnant women and young children. Lead in drinking water is primarily from materials and components associated with service lines and home plumbing. City of Dunn is responsible for providing high quality drinking water and removing lead pipes, but cannot control the variety of materials used in plumbing components in your home. You share the responsibility for protecting yourself and your family from the lead in your home plumbing. You can take responsibility by identifying and removing lead materials within your home plumbing and taking steps to reduce your family's risk. Before drinking tap water, flush your pipes for several minutes by running your tap, taking a shower, doing laundry or a load of dishes. You can also use a filter certified by an American National Standards Institute accredited certifier to reduce lead in drinking water. If you are concerned about lead in your water and wish to have your water tested, contact City of Dunn @ 910-897-5129. Information on lead in drinking water, testing methods, and steps you can take to minimize exposure is available at http://www.epa.gov/safewater/lead.
Total Trihalomethanes (TTHM) and Haloacetic Acids (five) (HAA5)
	
Disinfection Byproduct
	
Year Sampled
	
MCL Violation Y/N
	
Your Water
	Range

Low	High
	
MCLG
	
MCL
	
Likely Source of Contamination

	TTHM (ppb)
	2025
	N
	45 (ppb)
	23.3-40.6 (ppb)
	N/A
	80
	Byproduct of drinking water disinfection

	HAA5 (ppb)
	2025
	N
	39 (ppb)
	             18.6-44.6 (ppb)
	N/A
	60
	Byproduct of drinking water disinfection


Some people who drink water containing haloacetic acids in excess of the MCL over many years may have an increased risk of getting cancer.
Disinfectant Residuals Summary
	
	
MRDL
Violation Y/N
	Your Water (RAA)
	Range
Low	High
	
MRDLG
	
MRDL
	
Likely Source of Contamination

	Chlorine (ppm)
	N
	0.64 (ppm)
	0-3 (ppm)
	4
	4.0
	Water additive used to control microbes

	Chloramines (ppm)
	N
	2.44 (ppm)
	1.1-3.5 (ppm)
	
4
	
4.0
	Water additive used to control microbes



Inorganic Contaminants
	Contaminant (units)
	Sample Date
	MCL
Violation Y/N
	Your Water
	Range

Low	High
	
MCLG
	
MCL
	
Likely Source of Contamination

	Fluoride (ppm)
	1/7/25
	N
	0.61 (ppm)
	N/A
	4
	4
	Erosion of natural deposits; water additive which promotes strong teeth; discharge from fertilizer and aluminum factories


                                  

Turbidity*
	

Contaminant (units)
	Treatment Technique (TT)
Violation
Y/N
	

Your Water
	

MCLG
	

Treatment Technique (TT) Violation if:
	
Likely Source of Contamination

	Turbidity (NTU)  -  Highest single turbidity measurement
	N
	0.26                      NTU
	N/A
	
Turbidity  > 1  NTU

	Soil runoff

	Turbidity (%)  -  Lowest monthly percentage (%) of samples meeting turbidity limits
	N
	100 %
	N/A
	
Less than 95% of monthly turbidity measurements are <  0.3 NTU

	


 * Turbidity is a measure of the cloudiness of the water. We monitor it because it is a good indicator of the effectiveness of our filtration system. The turbidity rule requires that 95% or more of the monthly samples must be less than or equal to 0.3 NTU.
Total Organic Carbon (TOC)
	
Contaminant (units)
	TT
Violation Y/N
	Your Water (lowest RAA)
	Range Monthly Removal Ratio Low - High
	
MCLG
	
Treatment Technique (TT) violation if:
	
Likely Source of Contamination

	Total Organic Carbon (TOC) Removal Ratio (no units)

	N
	3.04
	0.95-1.42
	N/A
	Removal Ratio   RAA <1.00 and alternative compliance criteria was not met
	Naturally present in the environment



	
Contaminant (units)
	
Sample Date
	Your Water
	Range
Low	High
	
SMCL

	Sodium (ppm)
	1/7/25
	21.7 (ppm)
	N/A
	N/A

	Sulfate (ppm)
	1/7/25
	37.1 (ppm)
	N/A
	250

	pH
	1/7/25
	6.9
	N/A
	6.5 to 8.5


Other Miscellaneous Water Characteristics Contaminants
The PWS Section requires monitoring for other misc. contaminants, some for which the EPA has set national secondary drinking water standards (SMCLs) because they may cause cosmetic effects or aesthetic effects (such as taste, odor, and/or color) in drinking water.  The contaminants with SMCLs normally do not have any health effects and normally do not affect the safety of your water.
UCMR5 sampling 2023 Entry Point 1
	
Contaminant (units) ppb
	
Sample Date
	Your Water
	Range
Low	High

	perfluorobutanoic acid (PFBA)
	2023
	0.010 ppb
	0.007 - 0.013 ppb

	perfluoropentanoic acid (PFPeA)
	2023
	0.013 ppb
	0.008 - 0.022 ppb

	perfluorohexanoic acid (PFHxA)
	2023
	0.012 ppb
	0.008 – 0.020 ppb

	perfluoroheptanoic acid (PFHpA)
	2023
	0.005 ppb
	0.004 – 0.008 ppb

	perfluorooctanoic acid (PFOA)
	2023
	0.009 ppb
	0.006 – 0.012 ppb

	Perfluorobutanesulfonic acid (PFBS)
	2023
	0.008 ppb
	0.005 – 0.014 ppb

	Perfluorohexanesulfonic acid (PFHxS)
	2023
	0.004 ppb
	0.003 – 0.005 ppb

	Perfluorooctanesulfonic acid (PFOS)
	2023
	0.012 ppb
	    0.01- 0.014 ppb


	
Contaminant (units) ppb
	
Sample Date
	Your Water
	Range
Low	High

	perfluorobutanoic acid (PFBA)
	2024
	0.0070 ppb
	N/A

	perfluoropentanoic acid (PFPeA)
	2024
	0.0102 ppb
	N/A

	perfluorohexanoic acid (PFHxA)
	2024
	0.0110 ppb
	N/A

	perfluoroheptanoic acid (PFHpA)
	2024
	0.0047 ppb
	N/A

	perfluorooctanoic acid (PFOA)
	2024
	0.0087ppb
	N/A

	Perfluorobutanesulfonic acid (PFBS)
	2024
	0.0069 ppb
	N/A

	Perfluorohexanesulfonic acid (PFHxS)
	2024
	0.0040 ppb
	N/A

	Perfluorooctanesulfonic acid (PFOS)
	2024
	0.0129 ppb
	   N/A
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